# i386/x86_64 cpu features
config BR2_X86_CPU_HAS_MMX
	bool
config BR2_X86_CPU_HAS_SSE
	bool
config BR2_X86_CPU_HAS_SSE2
	bool
config BR2_X86_CPU_HAS_SSE3
	bool
config BR2_X86_CPU_HAS_SSSE3
	bool
config BR2_X86_CPU_HAS_SSE4
	bool
config BR2_X86_CPU_HAS_SSE42
	bool

choice
	prompt "Target Architecture Variant"
	depends on BR2_i386 || BR2_x86_64
	default BR2_x86_i586 if BR2_i386
	default BR2_x86_generic if BR2_x86_64
	help
	  Specific CPU variant to use

config BR2_x86_generic
	bool "generic"
config BR2_x86_i386
	bool "i386"
	depends on !BR2_x86_64
config BR2_x86_i486
	bool "i486"
	depends on !BR2_x86_64
config BR2_x86_i586
	bool "i586"
	depends on !BR2_x86_64
config BR2_x86_i686
	bool "i686"
	depends on !BR2_x86_64
config BR2_x86_pentiumpro
	bool "pentium pro"
	depends on !BR2_x86_64
config BR2_x86_pentium_mmx
	bool "pentium MMX"
	select BR2_X86_CPU_HAS_MMX
	depends on !BR2_x86_64
config BR2_x86_pentium_m
	bool "pentium mobile"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	depends on !BR2_x86_64
config BR2_x86_pentium2
	bool "pentium2"
	select BR2_X86_CPU_HAS_MMX
	depends on !BR2_x86_64
config BR2_x86_pentium3
	bool "pentium3"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	depends on !BR2_x86_64
config BR2_x86_pentium4
	bool "pentium4"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	select BR2_X86_CPU_HAS_SSE2
	depends on !BR2_x86_64
config BR2_x86_prescott
	bool "prescott"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	select BR2_X86_CPU_HAS_SSE2
	select BR2_X86_CPU_HAS_SSE3
	depends on !BR2_x86_64
config BR2_x86_nocona
	bool "nocona"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	select BR2_X86_CPU_HAS_SSE2
	select BR2_X86_CPU_HAS_SSE3
config BR2_x86_core2
	bool "core2"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	select BR2_X86_CPU_HAS_SSE2
	select BR2_X86_CPU_HAS_SSE3
	select BR2_X86_CPU_HAS_SSSE3
config BR2_x86_atom
	bool "atom"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	select BR2_X86_CPU_HAS_SSE2
	select BR2_X86_CPU_HAS_SSE3
	select BR2_X86_CPU_HAS_SSSE3
config BR2_x86_k6
	bool "k6"
	select BR2_X86_CPU_HAS_MMX
	depends on !BR2_x86_64
config BR2_x86_k6_2
	bool "k6-2"
	select BR2_X86_CPU_HAS_MMX
	depends on !BR2_x86_64
config BR2_x86_athlon
	bool "athlon"
	select BR2_X86_CPU_HAS_MMX
	depends on !BR2_x86_64
config BR2_x86_athlon_4
	bool "athlon-4"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	depends on !BR2_x86_64
config BR2_x86_opteron
	bool "opteron"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	select BR2_X86_CPU_HAS_SSE2
config BR2_x86_opteron_sse3
	bool "opteron w/ SSE3"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	select BR2_X86_CPU_HAS_SSE2
	select BR2_X86_CPU_HAS_SSE3
config BR2_x86_barcelona
	bool "barcelona"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	select BR2_X86_CPU_HAS_SSE2
	select BR2_X86_CPU_HAS_SSE3
config BR2_x86_jaguar
	bool "jaguar"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	select BR2_X86_CPU_HAS_SSE2
	select BR2_X86_CPU_HAS_SSE3
	select BR2_X86_CPU_HAS_SSSE3
	select BR2_X86_CPU_HAS_SSE4
	select BR2_X86_CPU_HAS_SSE42
config BR2_x86_geode
	bool "geode"
	# Don't include MMX support because there several variant of geode
	# processor, some with MMX support, some without.
	# See: http://en.wikipedia.org/wiki/Geode_%28processor%29
	depends on !BR2_x86_64
config BR2_x86_c3
	bool "Via/Cyrix C3 (Samuel/Ezra cores)"
	select BR2_X86_CPU_HAS_MMX
	depends on !BR2_x86_64
config BR2_x86_c32
	bool "Via C3-2 (Nehemiah cores)"
	select BR2_X86_CPU_HAS_MMX
	select BR2_X86_CPU_HAS_SSE
	depends on !BR2_x86_64
config BR2_x86_winchip_c6
	bool "IDT Winchip C6"
	select BR2_X86_CPU_HAS_MMX
	depends on !BR2_x86_64
config BR2_x86_winchip2
	bool "IDT Winchip 2"
	select BR2_X86_CPU_HAS_MMX
	depends on !BR2_x86_64
endchoice

config BR2_ARCH
	default "i386"		if BR2_x86_i386
	default "i486"		if BR2_x86_i486
	default "i586"		if BR2_x86_i586
	default "i586"		if BR2_x86_pentium_mmx
	default "i586"		if BR2_x86_geode
	default "i586"		if BR2_x86_c3
	default "i686"		if BR2_x86_c32
	default "i586"		if BR2_x86_winchip_c6
	default "i586"		if BR2_x86_winchip2
	default "i686"		if BR2_x86_i686
	default "i686"		if BR2_x86_pentium2
	default "i686"		if BR2_x86_pentium3
	default "i686"		if BR2_x86_pentium4
	default "i686"		if BR2_x86_pentium_m
	default "i686"		if BR2_x86_pentiumpro
	default "i686"		if BR2_x86_prescott
	default "i686"		if BR2_x86_nocona && BR2_i386
	default "i686"		if BR2_x86_core2 && BR2_i386
	default "i686"		if BR2_x86_atom && BR2_i386
	default "i686"		if BR2_x86_opteron && BR2_i386
	default "i686"		if BR2_x86_opteron_sse3 && BR2_i386
	default "i686"		if BR2_x86_barcelona && BR2_i386
	default "i686"		if BR2_x86_jaguar && BR2_i386
	default "i686"		if BR2_x86_k6
	default "i686"		if BR2_x86_k6_2
	default "i686"		if BR2_x86_athlon
	default "i686"		if BR2_x86_athlon_4
	default "x86_64"	if BR2_x86_64
	default "i386"		if BR2_x86_generic

config BR2_ENDIAN
	default "LITTLE"

config BR2_GCC_TARGET_TUNE
	default "i386"		if BR2_x86_i386
	default "i486"		if BR2_x86_i486
	default "i586"		if BR2_x86_i586
	default "pentium-mmx"	if BR2_x86_pentium_mmx
	default "i686"		if BR2_x86_i686
	default "pentiumpro"	if BR2_x86_pentiumpro
	default "pentium-m"	if BR2_x86_pentium_m
	default "pentium2"	if BR2_x86_pentium2
	default "pentium3"	if BR2_x86_pentium3
	default "pentium4"	if BR2_x86_pentium4
	default "prescott"	if BR2_x86_prescott
	default "nocona"	if BR2_x86_nocona
	default "core2"		if BR2_x86_core2
	default "atom"		if BR2_x86_atom
	default "k8"		if BR2_x86_opteron
	default "k8-sse3"	if BR2_x86_opteron_sse3
	default "barcelona"	if BR2_x86_barcelona
	default "btver2"	if BR2_x86_jaguar
	default "k6"		if BR2_x86_k6
	default "k6-2"		if BR2_x86_k6_2
	default "athlon"	if BR2_x86_athlon
	default "athlon-4"	if BR2_x86_athlon_4
	default "winchip-c6"	if BR2_x86_winchip_c6
	default "winchip2"	if BR2_x86_winchip2
	default "c3"		if BR2_x86_c3
	default "c3-2"		if BR2_x86_c32
	default "geode"		if BR2_x86_geode
	default "generic"	if BR2_x86_generic

config BR2_GCC_TARGET_ARCH
	default "i386"		if BR2_x86_i386
	default "i486"		if BR2_x86_i486
	default "i586"		if BR2_x86_i586
	default "pentium-mmx"	if BR2_x86_pentium_mmx
	default "i686"		if BR2_x86_i686
	default "pentiumpro"	if BR2_x86_pentiumpro
	default "pentium-m"	if BR2_x86_pentium_m
	default "pentium2"	if BR2_x86_pentium2
	default "pentium3"	if BR2_x86_pentium3
	default "pentium4"	if BR2_x86_pentium4
	default "prescott"	if BR2_x86_prescott
	default "nocona"	if BR2_x86_nocona
	default "core2"		if BR2_x86_core2
	default "atom"		if BR2_x86_atom
	default "k8"		if BR2_x86_opteron
	default "k8-sse3"	if BR2_x86_opteron_sse3
	default "barcelona"	if BR2_x86_barcelona
	default "btver2"	if BR2_x86_jaguar
	default "k6"		if BR2_x86_k6
	default "k6-2"		if BR2_x86_k6_2
	default "athlon"	if BR2_x86_athlon
	default "athlon-4"	if BR2_x86_athlon_4
	default "winchip-c6"	if BR2_x86_winchip_c6
	default "winchip2"	if BR2_x86_winchip2
	default "c3"		if BR2_x86_c3
	default "c3-2"		if BR2_x86_c32
	default "geode"		if BR2_x86_geode
