# Architecture
BR2_sh=y
BR2_sh4=y

# system
BR2_TARGET_GENERIC_GETTY=y
BR2_TARGET_GENERIC_GETTY_PORT="ttySC1"

# filesystem
BR2_TARGET_ROOTFS_EXT2=y
# BR2_TARGET_ROOTFS_TAR is not set

# Lock to 3.2 headers to avoid breaking with newer kernels
BR2_KERNEL_HEADERS_VERSION=y
BR2_DEFAULT_KERNEL_VERSION="3.2.53"

# The kernel wants to use the -m4-nofpu option to make sure that it
# doesn't use floating point operations.
BR2_EXTRA_GCC_CONFIG_OPTIONS="--with-multilib-list=m4,m4-nofpu"

# Linux kernel
BR2_LINUX_KERNEL=y
BR2_LINUX_KERNEL_CUSTOM_VERSION=y
BR2_LINUX_KERNEL_CUSTOM_VERSION_VALUE="3.2.53"
BR2_LINUX_KERNEL_USE_CUSTOM_CONFIG=y
BR2_LINUX_KERNEL_CUSTOM_CONFIG_FILE="board/qemu/sh4-r2d/linux-3.2.config"
BR2_LINUX_KERNEL_ZIMAGE=y
