From c12211a2f1832169e31063512b3e2081e503e856 Mon Sep 17 00:00:00 2001
From: Will Newton <will.newton@linaro.org>
Date: Tue, 2 Apr 2013 13:53:35 +0100
Subject: [PATCH 7/8] arm/clone.S: Add missing IT instruction for Thumb2.

The conditional load needs to be made part of an IT block on Thumb2
cores.

Signed-off-by: Will Newton <will.newton@linaro.org>
Signed-off-by: Thomas Petazzoni <thomas.petazzoni@free-electrons.com>
---
 libc/sysdeps/linux/arm/clone.S | 1 +
 1 file changed, 1 insertion(+)

diff --git a/libc/sysdeps/linux/arm/clone.S b/libc/sysdeps/linux/arm/clone.S
index e4101ba..1f7f09d 100644
--- a/libc/sysdeps/linux/arm/clone.S
+++ b/libc/sysdeps/linux/arm/clone.S
@@ -111,6 +111,7 @@ __clone:
 	ldr	r4, [sp, #12]
 	DO_CALL (clone)
 	movs	a1, a1
+	IT(t, ne)
 	ldmnefd	sp!, {r4}
 	blt	__error
 	IT(t, ne)
-- 
1.8.1.2

